**Product Name :English Breadboards 200x200mm to 300x1200mm**

**Description :**

● These solid aluminum, nonmagnetic baseplate form a high flatness breadboard by precision machined that provides a convenient and cost-effective platform for assembling small optical configuration, prototype set up, measurement system installation.
● Flatness ± 0.15mm over 0.3m²
● 1/4-20 through-tapped mounting holes on 1" centers, allowing components to be mounted on both sides at once.
● Four 8-32 counterbored holes and threaded holes separately located at corners for mounting pedestal or posts to increase height and more flexible applications.