**Product Name :Stainless Honeycomb Breadboards**

**Description :**

● Aluminum alloy precision formed honeycomb core.  
● Fast installation.  
● Machined Mat Finish on top surface.  
● All stainless steel side panels.  
● Steel-to-steel bonding throughout increase thermal stability.  
● Ferromagnetic stainless steel top skin 3 ~ 5 mm thick.  
● Ferromagnetic stainless steel bottom skin 3 ~ 4 mm thick.  
● Flatness: ± 0.1mm per 600 mm x 600 mm.  
● 10,000 class cleanroom compatible.