**Product Name :Stage Size 25x25mm Miniature Translation Stages**

**Description :**

● Linear crossed-roller bearing design for greater load capacity and high precision.  
● Compact and space-saving.  
● Rails in contact with cross-roller bearing are made of polished magnetism stainless steel to ensure long lasting smoothness and precision.  
● Travel range: 6mm in each direction.  
● Motion by micrometer in center is to easy read.  
● Minimum readout 0.01mm.  
● Left and right handed designs are available for convenience in alignment operation.  
● In use with adaptive plate 56LTS-AM allows fixation on breadboard or other mechanism components.  
● Aluminum Alloy material body and Magnetism stainless steel base combination.  
● Other translation arrangements are available on request.